## Power Efficiency Diagnostics Report

Computer Name | DESKTOP-063VVK1
Scan Time | 2026-08-18T11:55:57Z
Scan Duration | 60 seconds
System Manufacturer | AZW
System Product Name | MINI S
BIOS Date | 12/12/2023
BIOS Version | ADLNV105
OS Build | 26200
Platform Role | PlatformRoleMobile
Plugged In | true
Process Count | 215
Thread Count | 2308
Report GUID | {70609fbc-08a0-4565-afec-a4b40dbef126}

### Analysis Results

#### Errors

Power Policy:Sleep timeout is disabled (Plugged In)
The computer is not configured to automatically sleep after a period of inactivity.
System Availability Requests:System Required Request
A kernel component has made a request to prevent the system from automatically entering sleep.
USB Suspend:USB Device not Entering Selective Suspend
This device did not enter the USB Selective Suspend state. Processor power management may be prevented when this USB device is not in the Selective Suspend state. Note that this issue will not prevent the system from sleeping.

Device Name | USB Composite Device
Host Controller ID | PCI\VEN_8086&DEV_54ED
Host Controller Location | PCI bus 0, device 20, function 0
Device ID | USB\VID_062A&PID_385A
Port Path | 2

USB Suspend:USB Device not Entering Selective Suspend
This device did not enter the USB Selective Suspend state. Processor power management may be prevented when this USB device is not in the Selective Suspend state. Note that this issue will not prevent the system from sleeping.

Device Name | USB Mass Storage Device
Host Controller ID | PCI\VEN_8086&DEV_54ED
Host Controller Location | PCI bus 0, device 20, function 0
Device ID | USB\VID_1058&PID_25E2
Port Path | 15

CPU Utilization:Processor utilization is high
The average processor utilization during the trace was high. The system will consume less power when the average processor utilization is very low. Review processor utilization for individual processes to determine which applications and services contribute the most to total processor utilization.

Average Utilization (%) | 23.22

Platform Power Management Capabilities:Adaptive Display Brightness Support
This computer does not allow Windows to automatically control the brightness of the integrated display. Installing the latest system firmware (BIOS) may resolve this issue.
Platform Power Management Capabilities:PCI Express Active-State Power Management (ASPM) Disabled
PCI Express Active-State Power Management (ASPM) has been disabled due to a known incompatibility with the hardware in this computer.
Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Device
Device ID | PCI\VEN_8086&DEV_54C6&SUBSYS_72708086&REV_00\3&11583659&0&C9
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Device
Device ID | PCI\VEN_8086&DEV_54E8&SUBSYS_72708086&REV_00\3&11583659&0&A8
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | Unknown Device
Device ID | ACPI\INTC1023\2&DABA3FF&0
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Device
Device ID | PCI\VEN_8086&DEV_54C5&SUBSYS_72708086&REV_00\3&11583659&0&C8
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Simple Communications Controller
Device ID | PCI\VEN_8086&DEV_54A8&SUBSYS_72708086&REV_00\3&11583659&0&F0
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | Unknown Device
Device ID | ACPI\INTC1057\2&DABA3FF&0
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Device
Device ID | PCI\VEN_8086&DEV_54E9&SUBSYS_72708086&REV_00\3&11583659&0&A9
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | PCI Device
Device ID | PCI\VEN_8086&DEV_54AB&SUBSYS_72708086&REV_00\3&11583659&0&F3
Device Status | 0x1802400
Device Problem Code | 0x1c

Device Drivers:
Devices with missing or misconfigured drivers can increase power consumption.

Device Name | Unknown Device
Device ID | ACPI\INTC1024\2&DABA3FF&0
Device Status | 0x1802400
Device Problem Code | 0x1c

#### Warnings

Platform Timer Resolution:Outstanding Timer Request
A program or service has requested a timer resolution smaller than the platform maximum timer resolution.

Requested Period | 10000
Requesting Process ID | 3036
Requesting Process Path | \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe

Platform Timer Resolution:Outstanding Timer Request
A program or service has requested a timer resolution smaller than the platform maximum timer resolution.

Requested Period | 10000
Requesting Process ID | 4424
Requesting Process Path | \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | System
PID | 4
Average Utilization (%) | 5.55
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 1.85
\SystemRoot\System32\DriverStore\FileRepository\iigd_dch.inf_amd64_68fe65fbc646d3a4\igdkmdn64.sys | 1.51
\SystemRoot\System32\drivers\tcpip.sys | 0.47

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | caddy.exe
PID | 3840
Average Utilization (%) | 2.33
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 0.81
\Device\HarddiskVolume4\caddy\caddy.exe | 0.78
\SystemRoot\system32\drivers\NETIO.SYS | 0.32

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | Docker Desktop.exe
PID | 12760
Average Utilization (%) | 1.02
Module | Average Module Utilization (%)
\Device\HarddiskVolume4\Program Files\Docker\Docker\frontend\Docker Desktop.exe | 0.82
| 0.13
\SystemRoot\system32\ntoskrnl.exe | 0.05

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | parsecd.exe
PID | 4424
Average Utilization (%) | 0.94
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 0.60
\Device\HarddiskVolume4\Windows\System32\ntdll.dll | 0.16
\Device\HarddiskVolume4\Program Files\Parsec\verified\parsecd.dll | 0.05

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | MsMpEng.exe
PID | 2300
Average Utilization (%) | 0.71
Module | Average Module Utilization (%)
\Device\HarddiskVolume4\ProgramData\Microsoft\Windows Defender\Definition Updates\{8E1555F1-DFC7-4D29-93D1-944F742F4910}\mpengine.dll | 0.40
\SystemRoot\system32\ntoskrnl.exe | 0.16
\Device\HarddiskVolume4\Windows\System32\ntdll.dll | 0.06

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | python.exe
PID | 5340
Average Utilization (%) | 0.71
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 0.40
\Device\HarddiskVolume4\Users\Joe\AppData\Local\Programs\Python\Python313\python313.dll | 0.07
\SystemRoot\system32\drivers\afd.sys | 0.06

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | parsecd.exe
PID | 3036
Average Utilization (%) | 0.66
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 0.35
\Device\HarddiskVolume4\ProgramData\Parsec\parsecd-150-104a.dll | 0.10
\Device\HarddiskVolume4\Windows\System32\ntdll.dll | 0.09

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | vmmemWSL
PID | 8780
Average Utilization (%) | 0.57
Module | Average Module Utilization (%)
\SystemRoot\system32\ntoskrnl.exe | 0.49
\SystemRoot\System32\drivers\winhvr.sys | 0.02
| 0.02

CPU Utilization:Individual process with significant processor utilization.
This process is responsible for a significant portion of the total processor utilization recorded during the trace.

Process Name | com.docker.backend.exe
PID | 10548
Average Utilization (%) | 0.41
Module | Average Module Utilization (%)
\Device\HarddiskVolume4\Program Files\Docker\Docker\resources\com.docker.backend.exe | 0.23
\SystemRoot\system32\ntoskrnl.exe | 0.15
\Device\HarddiskVolume4\Windows\System32\ntdll.dll | 0.00

#### Information

Platform Timer Resolution:Platform Timer Resolution
The default platform timer resolution is 15.6ms (15625000ns) and should be used whenever the system is idle. If the timer resolution is increased, processor power management technologies may not be effective. The timer resolution may be increased due to multimedia playback or graphical animations.

Current Timer Resolution (100ns units) | 156250

Platform Timer Resolution:Timer Request Stack
The stack of modules responsible for the lowest platform timer setting in this process.

Requested Period | 10000
Requesting Process ID | 3036
Requesting Process Path | \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe
Calling Module Stack | \Device\HarddiskVolume4\Windows\System32\ntdll.dll
| \Device\HarddiskVolume4\Windows\System32\kernel32.dll
| \Device\HarddiskVolume4\ProgramData\Parsec\parsecd-150-104a.dll
| \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe
| \Device\HarddiskVolume4\Windows\System32\kernel32.dll
| \Device\HarddiskVolume4\Windows\System32\ntdll.dll

Platform Timer Resolution:Timer Request Stack
The stack of modules responsible for the lowest platform timer setting in this process.

Requested Period | 10000
Requesting Process ID | 4424
Requesting Process Path | \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe
Calling Module Stack | \Device\HarddiskVolume4\Windows\System32\ntdll.dll
| \Device\HarddiskVolume4\Windows\System32\kernel32.dll
| \Device\HarddiskVolume4\Program Files\Parsec\verified\parsecd.dll
| \Device\HarddiskVolume4\Program Files\Parsec\parsecd.exe
| \Device\HarddiskVolume4\Windows\System32\kernel32.dll
| \Device\HarddiskVolume4\Windows\System32\ntdll.dll

Power Policy:Active Power Plan
The current power plan in use

Plan Name | OEM Balanced
Plan GUID | {381b4222-f694-41f0-9685-ff5bb260df2e}

Power Policy:Power Plan Personality (On Battery)
The personality of the current power plan when the system is on battery power.

Personality | Balanced

Power Policy:Video Quality (On Battery)
Enables Windows Media Player to optimize for quality or power savings when playing video.

Quality Mode | Balance Video Quality and Power Savings

Power Policy:Power Plan Personality (Plugged In)
The personality of the current power plan when the system is plugged in.

Personality | Balanced

Power Policy:802.11 Radio Power Policy is Maximum Performance (Plugged In)
The current power policy for 802.11-compatible wireless network adapters is not configured to use low-power modes.
Power Policy:Video quality (Plugged In)
Enables Windows Media Player to optimize for quality or power savings when playing video.

Quality Mode | Optimize for Video Quality

Battery:Analysis Success
Analysis was successful. No energy efficiency problems were found. No information was returned.
Platform Power Management Capabilities:Supported Sleep States
Sleep states allow the computer to enter low-power modes after a period of inactivity. The S3 sleep state is the default sleep state for Windows platforms. The S3 sleep state consumes only enough power to preserve memory contents and allow the computer to resume working quickly. Very few platforms support the S1 or S2 Sleep states.

S1 Sleep Supported | false
S2 Sleep Supported | false
S3 Sleep Supported | true
S4 Sleep Supported | true

Platform Power Management Capabilities:Connected Standby Support
Connected standby allows the computer to enter a low-power mode in which it is always on and connected. If supported, connected standby is used instead of system sleep states.

Connected Standby Supported | false

Platform Power Management Capabilities:Processor Power Management Capabilities
Effective processor power management enables the computer to automatically balance performance and energy consumption.

Group | 0
Index | 0
Idle State Count | 3
Idle State Type | ACPI Idle (C) States
Nominal Frequency (MHz) | 800
Maximum Performance Percentage | 425
Lowest Performance Percentage | 100
Lowest Throttle Percentage | 12
Performance Controls Type | ACPI Collaborative Processor Performance Control

Platform Power Management Capabilities:Processor Power Management Capabilities
Effective processor power management enables the computer to automatically balance performance and energy consumption.

Group | 0
Index | 1
Idle State Count | 3
Idle State Type | ACPI Idle (C) States
Nominal Frequency (MHz) | 800
Maximum Performance Percentage | 425
Lowest Performance Percentage | 100
Lowest Throttle Percentage | 12
Performance Controls Type | ACPI Collaborative Processor Performance Control

Platform Power Management Capabilities:Processor Power Management Capabilities
Effective processor power management enables the computer to automatically balance performance and energy consumption.

Group | 0
Index | 2
Idle State Count | 3
Idle State Type | ACPI Idle (C) States
Nominal Frequency (MHz) | 800
Maximum Performance Percentage | 425
Lowest Performance Percentage | 100
Lowest Throttle Percentage | 12
Performance Controls Type | ACPI Collaborative Processor Performance Control

Platform Power Management Capabilities:Processor Power Management Capabilities
Effective processor power management enables the computer to automatically balance performance and energy consumption.

Group | 0
Index | 3
Idle State Count | 3
Idle State Type | ACPI Idle (C) States
Nominal Frequency (MHz) | 800
Maximum Performance Percentage | 425
Lowest Performance Percentage | 100
Lowest Throttle Percentage | 12
Performance Controls Type | ACPI Collaborative Processor Performance Control